[10:18:48 PM]:14    COM14     4.9960124s     resdump:<?xml version="1.0" encoding="UTF-8" ?>
<data>
<log value="ERROR: Only nop and sig tag can be recevied before authentication." /></data><?xml version="1.0" encoding="UTF-8" ?>
<data>
<response value="NAK" rawmode="false" /></data>


[10:20:35 PM]:14    COM14     4.9930188s     resdump:<?xml version="1.0" encoding="UTF-8" ?>
<data>
<log value="ERROR: Only nop and sig tag can be recevied before authentication." /></data><?xml version="1.0" encoding="UTF-8" ?>
<data>
<response value="NAK" rawmode="false" /></data>


[10:23:20 PM]:14    COM14     169.9898487s     Input string was not in a correct format.
[10:25:59 PM]:14    COM14     4.9957822s     resdump:<?xml version="1.0" encoding="UTF-8" ?>
<data>
<log value="ERROR: Only nop and sig tag can be recevied before authentication." /></data><?xml version="1.0" encoding="UTF-8" ?>
<data>
<response value="NAK" rawmode="false" /></data>


[10:28:49 PM]:14    COM14     174.9937363s     Input string was not in a correct format.
[10:35:03 PM]:14    COM14     5.0035581s     resdump:<?xml version="1.0" encoding="UTF-8" ?>
<data>
<log value="ERROR: Only nop and sig tag can be recevied before authentication." /></data><?xml version="1.0" encoding="UTF-8" ?>
<data>
<response value="NAK" rawmode="false" /></data>


[10:36:38 PM]:3    COM3     6.7213933s     resdump:<?xml version="1.0" encoding="UTF-8" ?>
<data>
<log value="ERROR: Only nop and sig tag can be recevied before authentication." /></data><?xml version="1.0" encoding="UTF-8" ?>
<data>
<response value="NAK" rawmode="false" /></data>


[10:37:08 PM]:14    COM14     130.0171299s     Input string was not in a correct format.
[10:37:23 PM]:3    COM3     51.722158s     Input string was not in a correct format.
[10:45:24 PM]:3    COM3     5.0032874s     resdump:<?xml version="1.0" encoding="UTF-8" ?>
<data>
<log value="ERROR: Only nop and sig tag can be recevied before authentication." /></data><?xml version="1.0" encoding="UTF-8" ?>
<data>
<response value="NAK" rawmode="false" /></data>


[10:45:29 PM]:3    COM3     4.8594973s     System.IO.IOException: The requested resource is in use.

   at System.IO.Ports.InternalResources.WinIOError(Int32 errorCode, String str)
   at System.IO.Ports.SerialStream..ctor(String portName, Int32 baudRate, Parity parity, Int32 dataBits, StopBits stopBits, Int32 readTimeout, Int32 writeTimeout, Handshake handshake, Boolean dtrEnable, Boolean rtsEnable, Boolean discardNull, Byte parityReplace)
   at System.IO.Ports.SerialPort.Open()
   at XiaoMiFlash.code.bl.SerialPortDevice.registerPort(SerialPort port)     at System.IO.Ports.InternalResources.WinIOError(Int32 errorCode, String str)
   at System.IO.Ports.SerialStream..ctor(String portName, Int32 baudRate, Parity parity, Int32 dataBits, StopBits stopBits, Int32 readTimeout, Int32 writeTimeout, Handshake handshake, Boolean dtrEnable, Boolean rtsEnable, Boolean discardNull, Byte parityReplace)
   at System.IO.Ports.SerialPort.Open()
   at XiaoMiFlash.code.bl.SerialPortDevice.registerPort(SerialPort port)
[10:45:49 PM]:3    COM3     24.8491877s     System.IO.IOException: The requested resource is in use.

   at System.IO.Ports.InternalResources.WinIOError(Int32 errorCode, String str)
   at System.IO.Ports.SerialStream..ctor(String portName, Int32 baudRate, Parity parity, Int32 dataBits, StopBits stopBits, Int32 readTimeout, Int32 writeTimeout, Handshake handshake, Boolean dtrEnable, Boolean rtsEnable, Boolean discardNull, Byte parityReplace)
   at System.IO.Ports.SerialPort.Open()
   at XiaoMiFlash.code.bl.SerialPortDevice.registerPort(SerialPort port)     at System.IO.Ports.InternalResources.WinIOError(Int32 errorCode, String str)
   at System.IO.Ports.SerialStream..ctor(String portName, Int32 baudRate, Parity parity, Int32 dataBits, StopBits stopBits, Int32 readTimeout, Int32 writeTimeout, Handshake handshake, Boolean dtrEnable, Boolean rtsEnable, Boolean discardNull, Byte parityReplace)
   at System.IO.Ports.SerialPort.Open()
   at XiaoMiFlash.code.bl.SerialPortDevice.registerPort(SerialPort port)
[10:46:24 PM]:3    COM3     9.9938847s     resdump:<?xml version="1.0" encoding="UTF-8" ?>
<data>
<log value="ERROR: Only nop and sig tag can be recevied before authentication." /></data><?xml version="1.0" encoding="UTF-8" ?>
<data>
<response value="NAK" rawmode="false" /></data>


[10:49:07 PM]:3    COM3     5.0036669s     resdump:<?xml version="1.0" encoding="UTF-8" ?>
<data>
<log value="ERROR: Only nop and sig tag can be recevied before authentication." /></data><?xml version="1.0" encoding="UTF-8" ?>
<data>
<response value="NAK" rawmode="false" /></data>


[10:52:11 PM]:3    COM3     5.0009632s     resdump:<?xml version="1.0" encoding="UTF-8" ?>
<data>
<log value="ERROR: Only nop and sig tag can be recevied before authentication." /></data><?xml version="1.0" encoding="UTF-8" ?>
<data>
<response value="NAK" rawmode="false" /></data>


[10:57:46 PM]:3    COM3     339.9969349s     System.Exception: authentication failed
   at XiaoMiFlash.code.bl.SerialPortDevice.dlAuth()
   at XiaoMiFlash.code.bl.SerialPortDevice.ConfigureDDR(Int32 intSectorSize, Int32 buffer_sectors, String ddrType, Int32 m_iSkipStorageInit)
   at XiaoMiFlash.code.bl.SerialPortDevice.XiaomiFlashNew()     at XiaoMiFlash.code.bl.SerialPortDevice.dlAuth()
   at XiaoMiFlash.code.bl.SerialPortDevice.ConfigureDDR(Int32 intSectorSize, Int32 buffer_sectors, String ddrType, Int32 m_iSkipStorageInit)
   at XiaoMiFlash.code.bl.SerialPortDevice.XiaomiFlashNew()
